# NIF File Format Documentation

NIF Objects | Compound Types | Enum Types | Basic Types | File Versions

## MultiTextureElement

### Attributes

Name | Type | Arg | Arr1 | Arr2 | Cond | Description | From | To
--- | --- | --- | --- | --- | --- | --- | --- | ---
Has Image | bool |  |  |  |  | Looks like a memory address, so probably a bool. |  |
Image | Ref<NiImage> |  |  |  | hasImage | Link to the texture image. |  |
Clamp? | TexClampMode |  |  |  | hasImage | May be texture clamp mode. |  |
Filter? | TexFilterMode |  |  |  | hasImage | May be texture filter mode. |  |
UV Set? | uint |  |  |  | hasImage | This may be the UV set counting from 1 instead of zero. |  |
PS2 L | short |  |  |  | hasImage | 0? | 3.03 | 10.2.0.0
PS2 K | short |  |  |  | hasImage | -75? | 3.03 | 10.2.0.0
Unknown Short 3 | short |  |  |  | hasImage | Unknown. Usually 0 but sometimes 257 | 3.03 |

### Found In

- NiMultiTextureProperty